Telehandler checklist
Date __________________________________   Time __________________________________
Site or location __________________________________   Operator name __________________________________
Machine make, model and unit number __________________________________   Hour meter reading __________________________________
Before you start (engine off)
	Item
	Pass
	Fail
	N/A

	Operator's manual and the load chart are in the cab and readable
	☐
	☐
	☐

	Cab frame, overhead guard and glass are intact
	☐
	☐
	☐

	Seat, seat belt and any restraint are in good condition
	☐
	☐
	☐

	Boom sections, wear pads and chains show no cracks, bends or wear
	☐
	☐
	☐

	Forks or attachment are undamaged, and the carriage latch locks fully
	☐
	☐
	☐

	Stabilizers or outriggers extend, retract and lock, where fitted
	☐
	☐
	☐

	Hydraulic hoses, cylinders and fittings are free of leaks
	☐
	☐
	☐

	Tires and wheels are in good condition, and lug nuts are tight
	☐
	☐
	☐

	Engine oil, coolant, hydraulic fluid and fuel levels are correct
	☐
	☐
	☐

	Mirrors, lights and warning labels are clean and undamaged
	☐
	☐
	☐



After you start (engine on)
	Item
	Pass
	Fail
	N/A

	Gauges and warning lights work, and none stay on
	☐
	☐
	☐

	Horn, back-up alarm and lights work
	☐
	☐
	☐

	Steering modes work: front, crab and four-wheel
	☐
	☐
	☐

	Service brake stops the machine, and the parking brake holds
	☐
	☐
	☐

	Boom lifts, extends, lowers and retracts smoothly, and holds when released
	☐
	☐
	☐

	Attachment tilt and any side-shift work smoothly
	☐
	☐
	☐

	Frame leveling works, where fitted
	☐
	☐
	☐

	Load moment indicator or load-limit warning works, where fitted
	☐
	☐
	☐

	No unusual noises, smells or vibration
	☐
	☐
	☐

	Fire extinguisher is in place, if your site requires one
	☐
	☐
	☐



Load and route
	Item
	Pass
	Fail
	N/A

	Load weight and its center are known and within the load chart for this reach and height
	☐
	☐
	☐

	Load is secure on the forks or attachment
	☐
	☐
	☐

	Ground is firm and level for the lift, with no soft spots or slopes
	☐
	☐
	☐

	Travel route is clear of people, power lines and overhead hazards
	☐
	☐
	☐

	Operator is trained on this machine and reads the load chart
	☐
	☐
	☐



Defects found and action taken
____________________________________________________________________________________________________
____________________________________________________________________________________________________
____________________________________________________________________________________________________
Taken out of service?  ☐ Yes   ☐ No        Reported to ______________________
Inspector signature __________________________________   Date __________________________________
Supervisor review __________________________________   Date __________________________________
A starting point. Adapt it to your equipment, your procedures and the rules that apply to you. Free template from portalbaseai.com
