Hot work permit
Permit no. __________________________________   Date __________________________________
Location __________________________________   Time permit starts __________________________________
Time permit ends __________________________________   Hot work to be done __________________________________
Person doing the work __________________________________   Fire watch __________________________________
Authorized by ______________________________________________________________________
Before the work starts
OSHA 1910.252 asks the person who authorizes cutting and welding to inspect the area and set the precautions, preferably in a written permit. Construction work has its own rules in 29 CFR 1926 Subpart J. Check the current text and your own program.
	☐ Area inspected by the person who authorizes the work
	☐ No explosive atmosphere, and no work in an area where one could form

	☐ Combustibles moved at least 35 feet (10.7 m) from the work, or shielded with flameproof covers or guards
	☐ Used containers cleaned and vented before any heat is applied

	☐ Floor swept clean for 35 feet, and wet or covered if it is combustible
	☐ Sprinklers in service, if the building has them

	☐ Floor and wall openings, cracks and open doorways covered so sparks cannot drop or travel
	☐ Fire extinguisher or hose ready for instant use

	☐ Ducts and conveyors that could carry sparks protected or shut down
	☐ Fire watch assigned, trained and holding a fire extinguisher

	☐ Combustible walls and partitions near the work shielded
	☐ Fire alarm location known to the welder and the fire watch



Special conditions
Anything specific to this job.
____________________________________________________________________________________________________
____________________________________________________________________________________________________
____________________________________________________________________________________________________
After the work
The fire watch stays for at least a half hour after welding or cutting stops, to catch smoldering fires.
	Work finished (time)
	Fire watch until (time)
	Area checked by
	Permit closed (initials)

	
	
	
	

	
	
	
	



A starting point. Adapt it to your equipment, your procedures and the rules that apply to you. Free template from portalbaseai.com
